IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Project Number"
Time stamp: "2022-04-15T09:36:48"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "22.0.2.392 - Exporter 22.4.2.0 - Alternate UI 22.4.2.0"
Application: "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)"

People and organizations
  Person "pablo.derendinger@engworks.com" of Organization (no name given)
  Owner history of Person "pablo.derendinger@engworks.com" of Organization (no name given) | application "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)" | change NOCHANGE | created 1650026123 (2022-04-15T12:35:23Z)

Units
  LENGTHUNIT: FOOT (conversion based)
  AREAUNIT: SQUARE FOOT (conversion based)
  VOLUMEUNIT: CUBIC FOOT (conversion based)
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  MASSFLOWRATEUNIT: derived
  ROTATIONALFREQUENCYUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  SOUNDPOWERUNIT: derived
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 31.181945″ | longitude -71° 3′ 24.263305″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "Boston", "MA"
      IFCBUILDINGSTOREY "Level 04 - T.O. Fnd. Wall" | long name "Level 04 - T.O. Fnd. Wall" | object type "Level:Story Level" | elevation -1.
        contains 1 element
          1 x IFCDOOR | type IFCDOORSTYLE "Single-Flush:36" x 168"" | object type "Single-Flush:36" x 168"" | names: "Single-Flush:36" x 168":280466" | material: materials ("Door - Frame", "Door - Frame", "Door - Panel") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Story Level" | elevation 0.
        contains 140 elements
          16 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:Generic - 8"" | object type "Basic Wall:Generic - 8"" | names: "Basic Wall:Generic - 8":279537", "Basic Wall:Generic - 8":279571", "Basic Wall:Generic - 8":279590" (+13 more) | material: layers "Basic Wall:Generic - 8"" ("Default Wall" 0.666666666666667) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          42 x IFCBEAM | type IFCBEAMTYPE "Glulam-Western Species:2.5x10.5" | object type "Glulam-Western Species:2.5x10.5" | names: "Glulam-Western Species:2.5x10.5:282355", "Glulam-Western Species:2.5x10.5:282813", "Glulam-Western Species:2.5x10.5:283085" (+39 more) | material: "Softwood, Lumber" | property sets: Pset_BeamCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          15 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "Pipe Types:Default" | object type "Pipe Types:Default" | names: "Pipe Types:Default:283743", "Pipe Types:Default:283766", "Pipe Types:Default:283819" (+12 more) | property sets: Pset_DistributionFlowElementCommon, Pset_DuctConnection, Pset_ElementShading, Pset_FlowSegmentDuctSegment, Pset_FlowSegmentPipeSegment, Pset_PipeConnection
          2 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Bend Long Sweep - PVC - Sch 40 - DWV:Standard" | object type "Bend Long Sweep - PVC - Sch 40 - DWV:Standard" | names: "Bend Long Sweep - PVC - Sch 40 - DWV:Standard:379841", "Bend Long Sweep - PVC - Sch 40 - DWV:Standard:380594" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_PipeFittingTypeCommon
          2 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Cleanout Two-Way - PVC - Sch 40 - DWV:Standard" | object type "Cleanout Two-Way - PVC - Sch 40 - DWV:Standard" | names: "Cleanout Two-Way - PVC - Sch 40 - DWV:Standard:380277", "Cleanout Two-Way - PVC - Sch 40 - DWV:Standard:412941" | material: materials ("<Unnamed>", "<Unnamed>", "<Unnamed>"); "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_PipeFittingTypeCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Concrete Slab - 6"" | object type "Floor:Concrete Slab - 6"" | FLOOR | names: "Floor:Concrete Slab - 6":380837" | material: layers "Floor:Concrete Slab - 6"" ("Concrete, Cast-in-Place gray" 0.5) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:Generic - 6"" | object type "Basic Wall:Generic - 6"" | names: "Basic Wall:Generic - 6":398006", "Basic Wall:Generic - 6":398217", "Basic Wall:Generic - 6":398551" (+1 more) | material: layers "Basic Wall:Generic - 6"" ("Default Wall" 0.5) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Fixed:36" x 48"" | object type "Fixed:36" x 48"" | names: "Fixed:36" x 48":399233" | material: materials ("Glass", "Sash", "Sash", "Sash") | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_WindowCommon
          2 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:STOREFRONT_TYPE SF7" | object type "Curtain Wall:STOREFRONT_TYPE SF7" | names: "Curtain Wall:STOREFRONT_TYPE SF7:401116", "Curtain Wall:STOREFRONT_TYPE SF7:401965" | parts: 32 IFCMEMBER, 10 IFCPLATE | property sets: Pset_CurtainWallCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Bend Long Sweep - PVC - Sch 40 - DWV:Standard" | object type "Bend Long Sweep - PVC - Sch 40 - DWV:Standard" | names: "Bend Long Sweep - PVC - Sch 40 - DWV:Standard:408140", "Bend Long Sweep - PVC - Sch 40 - DWV:Standard:422927" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_PipeFittingTypeCommon
          2 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Elbow - PVC - Sch 40:Standard" | object type "Elbow - PVC - Sch 40:Standard" | names: "Elbow - PVC - Sch 40:Standard:408741", "Elbow - PVC - Sch 40:Standard:408743" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_PipeFittingTypeCommon
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Elbow - PVC - Sch 40:Standard" | object type "Elbow - PVC - Sch 40:Standard" | names: "Elbow - PVC - Sch 40:Standard:408785" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_PipeFittingTypeCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Electrical Fixtures 1:Electrical Fixtures 1" | object type "Electrical Fixtures 1:Electrical Fixtures 1" | names: "Electrical Fixtures 1:Electrical Fixtures 1:410907" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Bend Long Sweep - PVC - Sch 40 - DWV:Standard" | object type "Bend Long Sweep - PVC - Sch 40 - DWV:Standard" | names: "Bend Long Sweep - PVC - Sch 40 - DWV:Standard:412763" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_PipeFittingTypeCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Electrical 2:Electrical 2" | object type "Electrical 2:Electrical 2" | names: "Electrical 2:Electrical 2:412837" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Electrical 1:Electrical 2" | object type "Electrical 1:Electrical 2" | names: "Electrical 1:Electrical 2:412873" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Bend Long Sweep - PVC - Sch 40 - DWV:Standard" | object type "Bend Long Sweep - PVC - Sch 40 - DWV:Standard" | names: "Bend Long Sweep - PVC - Sch 40 - DWV:Standard:413061" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_PipeFittingTypeCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Electrical Fixtures 2:Electrical Fixtures 2" | object type "Electrical Fixtures 2:Electrical Fixtures 2" | names: "Electrical Fixtures 2:Electrical Fixtures 2:413341" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid
          22 x IFCFLOWSEGMENT | type IFCCABLECARRIERSEGMENTTYPE "Conduit without Fittings:Rigid Nonmetallic Conduit (RNC Sch 80)" | object type "Conduit without Fittings:Rigid Nonmetallic Conduit (RNC Sch 80)" | names: "Conduit without Fittings:Rigid Nonmetallic Conduit (RNC Sch 80):414831", "Conduit without Fittings:Rigid Nonmetallic Conduit (RNC Sch 80):416375", "Conduit without Fittings:Rigid Nonmetallic Conduit (RNC Sch 80):416385" (+19 more) | property sets: Pset_DistributionFlowElementCommon, Pset_FlowSegmentDuctSegment, Pset_FlowSegmentPipeSegment, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "Conduit Elbow - without Fittings - RNC:Standard" | object type "Conduit Elbow - without Fittings - RNC:Standard" | names: "Conduit Elbow - without Fittings - RNC:Standard:416957" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:GWB on Mtl Stud" | object type "Compound Ceiling:GWB on Mtl Stud" | CEILING | names: "Compound Ceiling:GWB on Mtl Stud:420497" | material: layers "Compound Ceiling:GWB on Mtl Stud" ("Metal Stud Layer" 0.0520833333333333) | property sets: Pset_CoveringCommon, Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff
          8 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "RECESSED - DIRECT_INDIRECT - AVANTE 1X:1' x 4' (2 lamps)" | object type "RECESSED - DIRECT_INDIRECT - AVANTE 1X:1' x 4' (2 lamps)" | names: "RECESSED - DIRECT_INDIRECT - AVANTE 1X:1' x 4' (2 lamps):420553", "RECESSED - DIRECT_INDIRECT - AVANTE 1X:1' x 4' (2 lamps):420564", "RECESSED - DIRECT_INDIRECT - AVANTE 1X:1' x 4' (2 lamps):421713" (+5 more) | material: materials ("<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>"); "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "Conduit Elbow - without Fittings - RNC:Standard" | object type "Conduit Elbow - without Fittings - RNC:Standard" | names: "Conduit Elbow - without Fittings - RNC:Standard:422518" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          5 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "Conduit Body - Type L - Aluminum:Standard" | object type "Conduit Body - Type L - Aluminum:Standard" | names: "Conduit Body - Type L - Aluminum:Standard:422558", "Conduit Body - Type L - Aluminum:Standard:423508", "Conduit Body - Type L - Aluminum:Standard:423616" (+2 more) | material: materials ("<Unnamed>", "<Unnamed>", "<Unnamed>"); "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "Conduit Elbow - without Fittings - RNC:Standard" | object type "Conduit Elbow - without Fittings - RNC:Standard" | names: "Conduit Elbow - without Fittings - RNC:Standard:422991", "Conduit Elbow - without Fittings - RNC:Standard:423244" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "Conduit Body - Type L - Aluminum:Standard" | object type "Conduit Body - Type L - Aluminum:Standard" | names: "Conduit Body - Type L - Aluminum:Standard:423298", "Conduit Body - Type L - Aluminum:Standard:423330" | material: materials ("<Unnamed>", "<Unnamed>", "<Unnamed>"); "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "Conduit Junction Box - Tee - PVC:Standard" | object type "Conduit Junction Box - Tee - PVC:Standard" | names: "Conduit Junction Box - Tee - PVC:Standard:423432" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "Conduit Junction Box - Tee - PVC:Standard" | object type "Conduit Junction Box - Tee - PVC:Standard" | names: "Conduit Junction Box - Tee - PVC:Standard:423528" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
      IFCBUILDINGSTOREY "Roof" | long name "Roof" | object type "Level:1/4" Head" | elevation 20.
        contains 11 elements
          5 x IFCFLOWSEGMENT | type IFCCABLECARRIERSEGMENTTYPE "Conduit without Fittings:Rigid Nonmetallic Conduit (RNC Sch 80)" | object type "Conduit without Fittings:Rigid Nonmetallic Conduit (RNC Sch 80)" | names: "Conduit without Fittings:Rigid Nonmetallic Conduit (RNC Sch 80):408888", "Conduit without Fittings:Rigid Nonmetallic Conduit (RNC Sch 80):413431", "Conduit without Fittings:Rigid Nonmetallic Conduit (RNC Sch 80):413433" (+2 more) | property sets: Pset_DistributionFlowElementCommon, Pset_FlowSegmentDuctSegment, Pset_FlowSegmentPipeSegment, Pset_ProductRequirements, Pset_QuantityTakeOff
          3 x IFCFLOWSEGMENT | type IFCCABLECARRIERSEGMENTTYPE "Conduit without Fittings:Conduit" | object type "Conduit without Fittings:Conduit" | names: "Conduit without Fittings:Conduit:408901", "Conduit without Fittings:Conduit:410523", "Conduit without Fittings:Conduit:411112" | property sets: Pset_DistributionFlowElementCommon, Pset_FlowSegmentDuctSegment, Pset_FlowSegmentPipeSegment, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "Conduit Elbow - without Fittings - RNC:Standard" | object type "Conduit Elbow - without Fittings - RNC:Standard" | names: "Conduit Elbow - without Fittings - RNC:Standard:415916" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "Conduit Elbow - without Fittings - RNC:Standard" | object type "Conduit Elbow - without Fittings - RNC:Standard" | names: "Conduit Elbow - without Fittings - RNC:Standard:416592", "Conduit Elbow - without Fittings - RNC:Standard:416940" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff

Types
  IFCDOORSTYLE "Single-Flush:36" x 168"" | 1 occurrence | material: materials ("Door - Frame", "Door - Frame", "Door - Panel") | property sets: Single-Flush:36" x 168":280466, Single-Flush:36" x 168":280466:1, Pset_DoorCommon, Pset_ProductRequirements
  IFCWALLTYPE "Basic Wall:Generic - 8"" | STANDARD | 16 occurrences | material: layers "Basic Wall:Generic - 8"" ("Default Wall" 0.666666666666667) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_WallCommon
  IFCBEAMTYPE "Glulam-Western Species:2.5x10.5" | 42 occurrences | property sets: Pset_BeamCommon, Pset_ProductRequirements
  IFCPIPESEGMENTTYPE "Pipe Types:Default" | 15 occurrences | property sets: Pset_ProductRequirements
  IFCPIPEFITTINGTYPE "Bend Long Sweep - PVC - Sch 40 - DWV:Standard" | 2 occurrences | material: "<Unnamed>" | property sets: Pset_ProductRequirements
  IFCPIPEFITTINGTYPE "Cleanout Two-Way - PVC - Sch 40 - DWV:Standard" | 2 occurrences | material: materials ("<Unnamed>", "<Unnamed>", "<Unnamed>") | property sets: Pset_ProductRequirements
  IFCSLABTYPE "Floor:Concrete Slab - 6"" | FLOOR | 1 occurrence | material: layers "Floor:Concrete Slab - 6"" ("Concrete, Cast-in-Place gray" 0.5) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_SlabCommon
  IFCWALLTYPE "Basic Wall:Generic - 6"" | STANDARD | 4 occurrences | material: layers "Basic Wall:Generic - 6"" ("Default Wall" 0.5) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_WallCommon
  IFCWINDOWSTYLE "Fixed:36" x 48"" | 1 occurrence | material: materials ("Glass", "Sash", "Sash", "Sash") | property sets: Fixed:36" x 48":399233, Pset_ProductRequirements, Pset_WindowCommon
  IFCCURTAINWALLTYPE "Curtain Wall:STOREFRONT_TYPE SF7" | 2 occurrences | property sets: Pset_CurtainWallCommon, Pset_ProductRequirements
  IFCPIPEFITTINGTYPE "Bend Long Sweep - PVC - Sch 40 - DWV:Standard" | 2 occurrences | material: "<Unnamed>" | property sets: Pset_ProductRequirements
  IFCPIPEFITTINGTYPE "Elbow - PVC - Sch 40:Standard" | 2 occurrences | material: "<Unnamed>" | property sets: Pset_ProductRequirements
  IFCPIPEFITTINGTYPE "Elbow - PVC - Sch 40:Standard" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_ProductRequirements
  IFCBUILDINGELEMENTPROXYTYPE "Electrical Fixtures 1:Electrical Fixtures 1" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_ProductRequirements
  IFCPIPEFITTINGTYPE "Bend Long Sweep - PVC - Sch 40 - DWV:Standard" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_ProductRequirements
  IFCBUILDINGELEMENTPROXYTYPE "Electrical 2:Electrical 2" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_ProductRequirements
  IFCBUILDINGELEMENTPROXYTYPE "Electrical 1:Electrical 2" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_ProductRequirements
  IFCPIPEFITTINGTYPE "Bend Long Sweep - PVC - Sch 40 - DWV:Standard" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_ProductRequirements
  IFCBUILDINGELEMENTPROXYTYPE "Electrical Fixtures 2:Electrical Fixtures 2" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_ProductRequirements
  IFCCABLECARRIERSEGMENTTYPE "Conduit without Fittings:Rigid Nonmetallic Conduit (RNC Sch 80)" | CONDUITSEGMENT | 27 occurrences | property sets: Pset_ProductRequirements
  IFCCABLECARRIERFITTINGTYPE "Conduit Elbow - without Fittings - RNC:Standard" | 3 occurrences | material: "<Unnamed>" | property sets: Pset_ProductRequirements
  IFCCOVERINGTYPE "Compound Ceiling:GWB on Mtl Stud" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_ElementShading, Pset_ProductRequirements
  IFCLIGHTFIXTURETYPE "RECESSED - DIRECT_INDIRECT - AVANTE 1X:1' x 4' (2 lamps)" | 8 occurrences | material: materials ("<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>") | property sets: Pset_ProductRequirements
  IFCCABLECARRIERFITTINGTYPE "Conduit Elbow - without Fittings - RNC:Standard" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_ProductRequirements
  IFCCABLECARRIERFITTINGTYPE "Conduit Body - Type L - Aluminum:Standard" | 5 occurrences | material: materials ("<Unnamed>", "<Unnamed>", "<Unnamed>") | property sets: Pset_ProductRequirements
  IFCCABLECARRIERFITTINGTYPE "Conduit Elbow - without Fittings - RNC:Standard" | 2 occurrences | material: "<Unnamed>" | property sets: Pset_ProductRequirements
  IFCCABLECARRIERFITTINGTYPE "Conduit Body - Type L - Aluminum:Standard" | 2 occurrences | material: materials ("<Unnamed>", "<Unnamed>", "<Unnamed>") | property sets: Pset_ProductRequirements
  IFCCABLECARRIERFITTINGTYPE "Conduit Junction Box - Tee - PVC:Standard" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_ProductRequirements
  IFCCABLECARRIERFITTINGTYPE "Conduit Junction Box - Tee - PVC:Standard" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_ProductRequirements
  IFCCABLECARRIERSEGMENTTYPE "Conduit without Fittings:Conduit" | CONDUITSEGMENT | 3 occurrences | property sets: Pset_ProductRequirements
  IFCCABLECARRIERFITTINGTYPE "Conduit Elbow - without Fittings - RNC:Standard" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_ProductRequirements

Property sets
  Pset_ProductRequirements | properties | on 42 objects (42 IFCBEAM) | on 1 type object
    Category = "Structural Framing" (IFCLABEL)
  Pset_ProductRequirements | properties | on 32 objects (32 IFCMEMBER)
    Category = "Curtain Wall Mullions" (IFCLABEL)
  Pset_ProductRequirements | properties | on 30 objects (30 IFCFLOWSEGMENT) | on 2 type objects
    Category = "Conduits" (IFCLABEL)
  Pset_ProductRequirements | properties | on 29 objects (20 IFCWALLSTANDARDCASE, 7 IFCOPENINGELEMENT, 2 IFCCURTAINWALL) | on 3 type objects
    Category = "Walls" (IFCLABEL)
  Pset_ProductRequirements | properties | on 16 objects (16 IFCFLOWFITTING) | on 8 type objects
    Category = "Conduit Fittings" (IFCLABEL)
  Pset_ProductRequirements | properties | on 15 objects (15 IFCFLOWSEGMENT) | on 1 type object
    Category = "Pipes" (IFCLABEL)
  Pset_ProductRequirements | properties | on 11 objects (11 IFCFLOWFITTING) | on 7 type objects
    Category = "Pipe Fittings" (IFCLABEL)
  Pset_ProductRequirements | properties | on 10 objects (10 IFCPLATE)
    Category = "Curtain Panels" (IFCLABEL)
  Pset_ProductRequirements: 11 more contents on 21 objects not shown
  Pset_ElementShading | properties | on 22 objects (20 IFCWALLSTANDARDCASE, 1 IFCCOVERING, 1 IFCSLAB) | on 4 type objects
    Roughness = 3. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_ElementShading | properties | on 15 objects (15 IFCFLOWSEGMENT)
    Roughness = 0.0018 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_QuantityTakeOff | properties | on 42 objects (42 IFCBEAM)
    Reference = "2.5x10.5" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 32 objects (32 IFCMEMBER)
    Reference = "2" x 5" rectangular" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 27 objects (27 IFCFLOWFITTING)
    Reference = "Standard" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 27 objects (27 IFCFLOWSEGMENT)
    Reference = "Rigid Nonmetallic Conduit (RNC Sch 80)" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 16 objects (16 IFCWALLSTANDARDCASE)
    Reference = "Generic - 8"" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 15 objects (15 IFCFLOWSEGMENT)
    Reference = "Default" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 10 objects (10 IFCPLATE)
    Reference = "Glazed" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 9 objects (7 IFCOPENINGELEMENT, 2 IFCCURTAINWALL)
    Reference = "STOREFRONT_TYPE SF7" (IFCIDENTIFIER)
  Pset_QuantityTakeOff: 10 more contents on 23 objects not shown
  Pset_ReinforcementBarPitchOfWall | properties | on 16 objects (16 IFCWALLSTANDARDCASE)
    Reference = "Generic - 8"" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 4 objects (4 IFCWALLSTANDARDCASE)
    Reference = "Generic - 6"" (IFCLABEL)
  Pset_WallCommon | properties | on 16 objects (16 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Generic - 8"" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 4 objects (4 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Generic - 6"" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 2 type objects
    IsExternal = TRUE (IFCBOOLEAN)
  Pset_OpeningElementCommon | properties | on 7 objects (7 IFCOPENINGELEMENT)
    Reference = "STOREFRONT_TYPE SF7" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "36" x 168"" (IFCIDENTIFIER)
    ThermalTransmittance = 3.7021 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_DoorCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 3.7021 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_BeamCommon | properties | on 8 objects (8 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "2.5x10.5" (IFCIDENTIFIER)
    Slope = 1.2188752351313 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 11.7526592735432 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_BeamCommon | properties | on 8 objects (8 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "2.5x10.5" (IFCIDENTIFIER)
    Slope = 0.99634789650493 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 11.9809781239077 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_BeamCommon | properties | on 5 objects (5 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "2.5x10.5" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 9.33333333333333 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_BeamCommon | properties | on 4 objects (4 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "2.5x10.5" (IFCIDENTIFIER)
    Slope = 1.18730731572883 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 12.0650903954343 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_BeamCommon | properties | on 3 objects (3 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "2.5x10.5" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 26.9791666666667 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_BeamCommon | properties | on 2 objects (2 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "2.5x10.5" (IFCIDENTIFIER)
    Slope = 1.2188752351313 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 11.7526592735431 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "2.5x10.5" (IFCIDENTIFIER)
    Slope = 1.21887523513129 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 11.7526592735432 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "2.5x10.5" (IFCIDENTIFIER)
    Slope = 0.642252148936036 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 12.1666666666667 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_BeamCommon: 11 more contents on 10 objects not shown
  Pset_ReinforcementBarPitchOfBeam | properties | on 42 objects (42 IFCBEAM)
    Reference = "2.5x10.5" (IFCLABEL)
  Pset_DistributionFlowElementCommon | properties | on 27 objects (27 IFCFLOWFITTING)
    Reference = "Standard" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 27 objects (27 IFCFLOWSEGMENT)
    Reference = "Rigid Nonmetallic Conduit (RNC Sch 80)" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 15 objects (15 IFCFLOWSEGMENT)
    Reference = "Default" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 8 objects (8 IFCFLOWTERMINAL)
    Reference = "1' x 4' (2 lamps)" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 3 objects (3 IFCFLOWSEGMENT)
    Reference = "Conduit" (IFCIDENTIFIER)
  Pset_DuctConnection | properties | on 15 objects (15 IFCFLOWSEGMENT)
    ConnectionType = ["Generic"] (IFCTEXT)
  Pset_FlowSegmentDuctSegment | properties | on 3 objects (3 IFCFLOWSEGMENT)
    Length = 7.16666666666667 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_FlowSegmentDuctSegment | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Length = 43.625 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_FlowSegmentDuctSegment | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Length = 1.41666666666667 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_FlowSegmentDuctSegment | properties | on 1 object (1 IFCFLOWSEGMENT)
    Length = 6. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_FlowSegmentDuctSegment | properties | on 1 object (1 IFCFLOWSEGMENT)
    Length = 6.10937500000003 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_FlowSegmentDuctSegment | properties | on 1 object (1 IFCFLOWSEGMENT)
    Length = 6.56908491611408 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_FlowSegmentDuctSegment | properties | on 1 object (1 IFCFLOWSEGMENT)
    Length = 5.25902439509091 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_FlowSegmentDuctSegment | properties | on 1 object (1 IFCFLOWSEGMENT)
    Length = 0.545622297349823 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_FlowSegmentDuctSegment: 33 more contents on 33 objects not shown
  Pset_FlowSegmentPipeSegment | properties | on 3 objects (3 IFCFLOWSEGMENT)
    Length = 7.16666666666667 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_FlowSegmentPipeSegment | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Length = 43.625 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_FlowSegmentPipeSegment | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Length = 1.41666666666667 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_FlowSegmentPipeSegment | properties | on 1 object (1 IFCFLOWSEGMENT)
    InvertElevation = 4.64635522757668 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Length = 6. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_FlowSegmentPipeSegment | properties | on 1 object (1 IFCFLOWSEGMENT)
    InvertElevation = 4.75202640252044 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Length = 6.10937500000003 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_FlowSegmentPipeSegment | properties | on 1 object (1 IFCFLOWSEGMENT)
    InvertElevation = 11.2454054534223 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Length = 6.56908491611408 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_FlowSegmentPipeSegment | properties | on 1 object (1 IFCFLOWSEGMENT)
    InvertElevation = 5.59639266126712 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Length = 5.25902439509091 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_FlowSegmentPipeSegment | properties | on 1 object (1 IFCFLOWSEGMENT)
    InvertElevation = 11.2449723502546 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Length = 0.545622297349823 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_FlowSegmentPipeSegment: 33 more contents on 33 objects not shown
  Pset_PipeConnection | properties | on 15 objects (15 IFCFLOWSEGMENT)
    ConnectionType = ["Generic"] (IFCLABEL)
  Pset_PipeFittingTypeCommon | properties | on 11 objects (11 IFCFLOWFITTING)
    NominalDiameter = [0.333333333333333] (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB)
    Reference = "Concrete Slab - 6"" (IFCLABEL)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Concrete Slab - 6"" (IFCIDENTIFIER)
    ThermalTransmittance = 6.86351706036745 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 6.86351706036745 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "36" x 48"" (IFCIDENTIFIER)
    ThermalTransmittance = 3.6886 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WindowCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 3.6886 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_CurtainWallCommon | properties | on 2 objects (2 IFCCURTAINWALL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "STOREFRONT_TYPE SF7" (IFCIDENTIFIER)
  Pset_CurtainWallCommon | properties | on 1 type object
    IsExternal = TRUE (IFCBOOLEAN)
  Pset_PlateCommon | properties | on 10 objects (10 IFCPLATE)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Glazed" (IFCIDENTIFIER)
    ThermalTransmittance = 6.7069 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_MemberCommon | properties | on 12 objects (12 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "2" x 5" rectangular" (IFCIDENTIFIER)
    Span = 1.56770455954539 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_MemberCommon | properties | on 6 objects (6 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "2" x 5" rectangular" (IFCIDENTIFIER)
    Span = 4. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_MemberCommon | properties | on 6 objects (6 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "2" x 5" rectangular" (IFCIDENTIFIER)
    Span = 4.07018826500516 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_MemberCommon | properties | on 2 objects (2 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "2" x 5" rectangular" (IFCIDENTIFIER)
    Span = 4.00000000000011 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_MemberCommon | properties | on 2 objects (2 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "2" x 5" rectangular" (IFCIDENTIFIER)
    Span = 3.99999999999988 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_MemberCommon | properties | on 2 objects (2 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "2" x 5" rectangular" (IFCIDENTIFIER)
    Span = 4.07018826500497 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_MemberCommon | properties | on 2 objects (2 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "2" x 5" rectangular" (IFCIDENTIFIER)
    Span = 3.57018826500533 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_BuildingElementProxyCommon | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Reference = "Electrical 2" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Electrical Fixtures 1" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Electrical Fixtures 2" (IFCIDENTIFIER)
  Pset_ProvisionForVoid | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Depth = 5.84273496032079 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_ProvisionForVoid | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Depth = 4.58333333333333 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    Height = 0.550435181280692 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    Width = 1.58640479869604 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_ProvisionForVoid | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Depth = 1.94877089077119 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    Height = 1.63507031942675 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    Width = 0.492343486423735 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_CoveringCommon | properties | on 1 object (1 IFCCOVERING)
    Reference = "GWB on Mtl Stud" (IFCIDENTIFIER)
    TotalThickness = 0.0520833333333333 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_CoveringCommon | properties | on 1 type object
    TotalThickness = 0.0520833333333333 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 04 - T.O. Fnd. Wall" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Roof" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 3 objects (3 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 3 (IFCINTEGER)
  Single-Flush:36" x 168":280466 | predefined | on 1 type object
  Single-Flush:36" x 168":280466:1 | predefined | on 1 type object
  Fixed:36" x 48":399233 | predefined | on 1 type object